R1 1M

C1 10n C2 10n

R3 1M

-70V

VbiasRet

Vbias 1

2

3

4

T1

IbiasHK

R11 1M C11 10n

R4 1M C4 10n D4 4.5V

R2 1M

+2V/uA

RSH REB GND

FILE: REVISION: DRAWN BY:

PAGE OF

TITLE Bias supply filters and current monitor

MSL RAD

bias_filter.sch 1 1 $Revision: 1.1 $ Stephan I. Böttcher